,"18"" Direct##other##","24"" Direct##other##","18"" Direct/Indirect##other##",Input Wattage##other##,Luminous Flux##other##,Initial Color Temperature##COLOR_TEMPERATURE##KELVIN,Body Finish##other##,Photometric Web File##other##
WRPP1P18-CR80-CTA40-FA01-DL00,1,0,0,22.4,3262,4000,Metal - Betacalco - White,WRPP1P18-CR80-CTA40-FA01-DL00.ies
WRPP1P24-CR80-CTA40-FA01-DL00,0,1,0,33.6,4873,4000,Metal - Betacalco - White,WRPP1P24-CR80-CTA40-FA01-DL00.ies
WRPP2P18-CR80-CTA40-UD2-FA01-DL00,0,0,1,43.2,5665,4000,Metal - Betacalco - White,WRPP2P18-CR80-CTA40-UD2-FA01-DL00.IES
WRPP2P24-CR80-CTA40-UD2-FA01-DL00,0,0,0,54.4,7174,4000,Metal - Betacalco - White,WRPP2P24-CR80-CTA40-UD2-FA01-DL00.ies
WRPP1P18-CR80-CTA40-FA01-DL40,1,0,0,50,5217,4000,Metal - Betacalco - White,WRPP1P18-CR80-CTA40-FA01-DL40.ies
WRPP1P24-CR80-CTA40-FA01-DL40,0,1,0,61.2,6723,4000,Metal - Betacalco - White,WRPP1P24-CR80-CTA40-FA01-DL40.ies
WRPP2P18-CR80-CTA40-UD2-FA01-DL40,0,0,1,70.7,7810,4000,Metal - Betacalco - White,WRPP2P18-CR80-CTA40-UD2-FA01-DL40.IES
WRPP2P24-CR80-CTA40-UD2-FA01-DL40,0,0,0,81.9,9014,4000,Metal - Betacalco - White,WRPP2P24-CR80-CTA40-UD2-FA01-DL40.ies
